# Cheatsheets

## CircuitBreakerOptions

Circuit breaker configuration options. All time are given in milliseconds.

Name | Type | Description
`fallbackOnFailure` | `Boolean` | Sets whether or not the fallback is executed on failure, even when the circuit is closed.
`maxFailures` | `Number (int)` | Sets the maximum number of failures before opening the circuit.
`notificationAddress` | `String` | Sets the event bus address on which the circuit breaker publish its state change.
`notificationPeriod` | `Number (long)` | Configures the period in milliseconds where the circuit breaker send a notification on the event bus with its current state.
`resetTimeout` | `Number (long)` | Sets the time in ms before it attempts to re-close the circuit (by going to the hal-open state). If the cricuit is closed when the timeout is reached, nothing happens. `-1` disables this feature.
`timeout` | `Number (long)` | Sets the timeout in milliseconds. If an action is not completed before this timeout, the action is considered as a failure.